## Technical specifications

**Gasoline engines**

|  |
| --- |
| **1.0 T-GDI** |
| Type | Kappa 1.0 T-GDI, 12-valve MLA, DOHC, three cylinder in-line |
| Capacity | 998 cc |
| Bore x stroke | 71 x 84.0 mm |
| Compression ratio | 10.0 |
| Power | 120 PS (88 kW) @ 6,000 rpm |
| Torque | 172 Nm @ 1,500~4,000 rpm |
| Maximum speed (km/h) | 181 km/h |
| 0-100 km/h (seconds) | 12.0 |
| CO2 combined (g/km)\* | 117 (16” wheels), 125 (17” and 18” wheels) |
| Fuel Consumption combined (l/100km)\* | 5.2 (16” wheels), 5.4 (17” and 18” wheels) |

|  |
| --- |
| **1.6 T-GDI** |
| Type | Gamma 1.6 T-GDI, 16-valve MLA, DOHC, four cylinder in-line |
| Capacity | 1,591 cc |
| Bore x stroke | 77 x 85.44 mm |
| Compression ratio | 10.0 |
| Power | 177 PS (130 kW) @ 5,500 rpm |
| Torque | 265 Nm @ 1,500~4,500 rpm |
| Maximum speed (km/h) | 205 km/h |
| 0-100 km/h (seconds) | 7.9 |
| CO2 combined (g/km)\* | 153 (17” and 18” wheels) |
| Fuel Consumption combined (l/100km)\* | 6.7 (17” and 18” wheels) |

**Transmissions**

Gasoline engines - speeds

|  |  |  |
| --- | --- | --- |
| **Engine** | **1.0 T-GDI (120 PS)** | **1.6 T-GDI (177 PS)** |
| Manual | 6 (with 2WD) | - |
| DCT | - | 7 (with 4WD) |

**Gear ratios**

|  |  |  |
| --- | --- | --- |
|  | **1.0 T-GDI (120 PS)** | **1.6 T-GDI (177 PS)** |
| **6MT** | **7DCT** |
| 1st | 3.769 | 3.643 |
| 2nd | 2.045 | 2.174 |
| 3rd | 1.286 | 1.826 |
| 4th | 0.971 | 1.024 |
| 5th  | 0.774 | 0.809 |
| 6th  | 0.639 | 0.854 |
| 7th  | - | 0.717 |
| Rev. | 3.700 | 4.696 |
| Final drive | 4.563 | 4.643 (1/2/4/5)3.611 (3/6/7/R) |

**Wheels and tyres**

|  |  |
| --- | --- |
| **Wheel type**  | **Tyres** |
| 16 inch steel / alloy | 205 / 60R16 |
| 17 inch alloy | 215 / 55R17 |
| 18 inch alloy | 235 / 45R18 |

**Dimensions (mm)**

|  |
| --- |
| **Exterior** |
| Overall length | 4,165  |
| Overall width | 1,800  |
| Overall height | 1,5501,565 (with roof rack) |
| Wheelbase | 2,600 |
| Front overhang | 845 |
| Rear overhang | 720 |
| Ground clearance | 170 |

|  |  |  |
| --- | --- | --- |
| **Interior** | **Front** | **Rear** |
| Head room | 1,005965 (with sunroof) | 961 |
| Leg room | 1,054 | 880 |
| Shoulder room | 1,409 | 1,385 |

**Cargo space (litres)**

|  |  |
| --- | --- |
| Luggage | 361 l (Minimum, VDA 211)  |
| 1,143 l Maximum, VDA 214)  |

**Weights (kg)\*\***

|  |  |
| --- | --- |
|  | **Gasoline** |
|  | **1.0 T-GDI** | **1.6 T-GDI** |
| Minimum Curb weight (without driver) | 1,233 | 1,401 |

*\* Based on NEDC Test Cycle. Fuel Consumption and emission values vary depending on tire size and transmission type.
\*\*Manufacturer’s estimates*